<?xml version="1.0" encoding="UTF-8"?>
<SCL xmlns="http://www.iec.ch/61850/2003/SCL" revision="A" version="2007">
  <Header id="" nameStructure="IEDName" toolID="FUHUA Model Designer ICT">
    <History>
      <Hitem revision="" version="" when="" />
    </History>
  </Header>
  <Communication>
    <SubNetwork name="W1">
      <ConnectedAP apName="AP1" iedName="IED1">
        <Address>
          <P type="OSI-AP-Title">1,1,1,999,1</P>
          <P type="OSI-AE-Qualifier">12</P>
          <P type="OSI-PSEL">00000001</P>
          <P type="OSI-SSEL">0001</P>
          <P type="OSI-TSEL">0001</P>
          <P type="IP">0.0.0.0</P>
          <P type="IP-SUBNET">255.255.255.0</P>
          <P type="IP-GATEWAY">0.0.0.0</P>
        </Address>
      </ConnectedAP>
    </SubNetwork>
  </Communication>
  <IED name="IED1" originalSclRevision="B" originalSclVersion="2007">
    <Services nameLength="64">
      <ClientServices />
      <ConfDataSet max="50" maxAttributes="100" />
      <ConfReportControl max="50" />
      <ReportSettings bufTime="Dyn" cbName="Conf" datSet="Conf" intgPd="Dyn" optFields="Dyn" trgOps="Dyn" />
      <ConfLNs fixLnInst="true" fixPrefix="true" />
      <DynAssociation />
      <GetDirectory />
      <GetDataObjectDefinition />
      <GetCBValues />
      <DataObjectDirectory />
      <GetDataSetValue />
      <DataSetDirectory />
      <ReadWrite />
      <GSESettings appID="Conf" cbName="Conf" datSet="Conf" />
      <GOOSE max="10" />
    </Services>
    <AccessPoint name="AP1">
      <Server>
        <Authentication none="true" />
        <LDevice inst="LD1">
          <LN0 inst="" lnClass="LLN0" lnType="LLN0_0">
            <DataSet name="AnalogEvents">
              <FCDA doName="AnIn1" fc="MX" ldInst="LD1" prefix="AnIn" lnClass="GGIO" lnInst="1" />
              <FCDA doName="AnIn2" fc="MX" ldInst="LD1" prefix="AnIn" lnClass="GGIO" lnInst="1" />
              <FCDA doName="AnIn3" fc="MX" ldInst="LD1" prefix="AnIn" lnClass="GGIO" lnInst="1" />
              <FCDA doName="AnIn4" fc="MX" ldInst="LD1" prefix="AnIn" lnClass="GGIO" lnInst="1" />
            </DataSet>
            <ReportControl bufTime="0" buffered="true" confRev="1" datSet="AnalogEvents" intgPd="5000" name="BRCB_Events">
              <TrgOps dchg="true" dupd="false" period="false" qchg="true" />
              <OptFields configRef="true" dataRef="true" dataSet="false" entryID="true" reasonCode="true" seqNum="true" timeStamp="true" />
              <RptEnabled max="2" />
            </ReportControl>
            <ReportControl bufTime="0" buffered="false" confRev="1" datSet="AnalogEvents" intgPd="5000" name="URCB_Events">
              <TrgOps dchg="true" dupd="false" period="false" qchg="true" />
              <OptFields configRef="true" dataRef="true" dataSet="false" reasonCode="true" seqNum="true" timeStamp="true" />
              <RptEnabled max="2" />
            </ReportControl>
            <DOI name="Mod">
              <DAI name="stVal">
                <Val>on</Val>
              </DAI>
            </DOI>
          </LN0>
          <LN inst="1" lnClass="LPHD" lnType="LPHD" />
          <LN inst="1" prefix="AnIn" lnClass="GGIO" lnType="GGIO_AnIn_MV">
            <DOI name="Beh">
              <DAI name="stVal">
                <Val>on</Val>
              </DAI>
            </DOI>
            <DOI name="AnIn1">
              <DAI name="db">
                <Val>10000</Val>
              </DAI>
              <DAI name="dbRef">
                <Val>10</Val>
              </DAI>
              <DAI name="zeroDb">
                <Val>1000</Val>
              </DAI>
              <DAI name="zeroDbRef">
                <Val>10</Val>
              </DAI>
            </DOI>
            <DOI name="AnIn2">
              <DAI name="db">
                <Val>1000</Val>
              </DAI>
              <DAI name="dbRef">
                <Val>10</Val>
              </DAI>
              <DAI name="zeroDb">
                <Val>1000</Val>
              </DAI>
              <DAI name="zeroDbRef">
                <Val>10</Val>
              </DAI>
            </DOI>
            <DOI name="AnIn3">
              <DAI name="db">
                <Val>10000</Val>
              </DAI>
              <DAI name="zeroDb">
                <Val>1000</Val>
              </DAI>
              <SDI name="rangeC">
                <SDI name="min">
                  <DAI name="f">
                    <Val>-5</Val>
                  </DAI>
                </SDI>
                <SDI name="max">
                  <DAI name="f">
                    <Val>5</Val>
                  </DAI>
                </SDI>
              </SDI>
            </DOI>
            <DOI name="AnIn4">
              <DAI name="db">
                <Val>1000</Val>
              </DAI>
              <DAI name="zeroDb">
                <Val>1000</Val>
              </DAI>
              <SDI name="rangeC">
                <SDI name="min">
                  <DAI name="f">
                    <Val>-100</Val>
                  </DAI>
                </SDI>
                <SDI name="max">
                  <DAI name="f">
                    <Val>100</Val>
                  </DAI>
                </SDI>
              </SDI>
            </DOI>
          </LN>
        </LDevice>
      </Server>
    </AccessPoint>
  </IED>
  <DataTypeTemplates>
    <LNodeType id="LPHD" lnClass="LPHD">
      <DO name="PhyNam" type="DPL" />
      <DO name="PhyHealth" type="ENS_Health" />
      <DO name="Proxy" type="SPS" />
    </LNodeType>
    <LNodeType id="LLN0_0" lnClass="LLN0">
      <DO name="Mod" type="ENC_Mod" />
      <DO name="Beh" type="ENS_Beh" />
      <DO name="Health" type="ENS_Health" />
      <DO name="NamPlt" type="LPL_NamPlt" />
    </LNodeType>
    <LNodeType id="GGIO_AnIn_MV" lnClass="GGIO">
      <DO name="Beh" type="ENS_Beh" />
      <DO name="AnIn1" type="MV_db" />
      <DO name="AnIn2" type="MV_db" />
      <DO name="AnIn3" type="MV_db_rangeC" />
      <DO name="AnIn4" type="MV_db_rangeC" />
    </LNodeType>
    <DOType cdc="DPL" id="DPL">
      <DA bType="VisString255" fc="DC" name="vendor" />
      <DA bType="VisString255" fc="DC" name="hwRev" />
      <DA bType="VisString255" fc="DC" name="swRev" />
      <DA bType="VisString255" fc="DC" name="serNum" />
      <DA bType="VisString255" fc="DC" name="model" />
      <DA bType="VisString255" fc="DC" name="location" />
      <DA bType="VisString64" fc="DC" name="name" />
      <DA bType="VisString255" fc="DC" name="owner" />
    </DOType>
    <DOType cdc="ENS" id="ENS_TmSyn">
      <DA bType="Enum" fc="ST" name="stVal" type="TmSynEnum" />
      <DA bType="Quality" fc="ST" name="q" />
      <DA bType="Timestamp" fc="ST" name="t" />
    </DOType>
    <DOType cdc="ENS" id="ENS_Beh">
      <DA bType="Enum" fc="ST" name="stVal" type="BehKind" />
      <DA bType="Quality" fc="ST" name="q" />
      <DA bType="Timestamp" fc="ST" name="t" />
    </DOType>
    <DOType cdc="SPS" id="SPS">
      <DA bType="BOOLEAN" dchg="true" fc="ST" name="stVal" />
      <DA bType="Quality" fc="ST" name="q" qchg="true" />
      <DA bType="Timestamp" fc="ST" name="t" />
      <DA bType="VisString255" fc="DC" name="d" />
    </DOType>
    <DOType cdc="ENC" id="ENC_Mod">
      <DA bType="Enum" dchg="true" fc="ST" name="stVal" type="ModKind" />
      <DA bType="Quality" fc="ST" name="q" qchg="true" />
      <DA bType="Timestamp" fc="ST" name="t" />
      <DA bType="Enum" fc="CF" name="ctlModel" type="ctlModel" />
    </DOType>
    <DOType cdc="ENC" id="ENC">
      <DA bType="Struct" fc="CO" name="Oper" type="ENCOperate" />
      <DA bType="VisString129" fc="CO" name="SBO" />
      <DA bType="Struct" fc="CO" name="SBOw" type="ENCOperate" />
      <DA bType="Struct" fc="ST" name="origin" type="Originator" />
      <DA bType="INT8U" fc="ST" name="ctlNum" />
      <DA bType="Enum" dchg="true" fc="ST" name="stVal" type="tempEnum" />
      <DA bType="Quality" fc="ST" name="q" qchg="true" />
      <DA bType="Timestamp" fc="ST" name="t" />
      <DA bType="Enum" fc="CF" name="ctlModel" type="ctlModel" />
    </DOType>
    <DOType cdc="INS" id="INS">
      <DA bType="INT32" dchg="true" fc="ST" name="stVal" />
      <DA bType="Quality" fc="ST" name="q" qchg="true" />
      <DA bType="Timestamp" fc="ST" name="t" />
      <DA bType="INT32U" fc="CF" name="db" />
      <DA bType="INT32U" fc="CF" name="zeroDb" />
    </DOType>
    <DOType cdc="MV" id="MV_db">
      <DA bType="Struct" fc="MX" name="instMag" type="AnalogueValue"/>
      <DA bType="Struct" dchg="true" dupd="false" fc="MX" name="mag" type="AnalogueValue" />
      <DA bType="Quality" fc="MX" name="q" qchg="true" />
      <DA bType="Timestamp" fc="MX" name="t" />
      <DA bType="INT32U" dchg="true" fc="CF" name="db" />
      <DA bType="INT32U" dchg="true" fc="CF" name="zeroDb" />
      <DA bType="FLOAT32" dchg="true" fc="CF" name="dbRef" />
      <DA bType="FLOAT32" dchg="true" fc="CF" name="zeroDbRef" />
    </DOType>
    <DOType cdc="MV" id="MV_db_rangeC">
      <DA bType="Struct" fc="MX" name="instMag" type="AnalogueValue"/>
      <DA bType="Struct" dchg="true" dupd="false" fc="MX" name="mag" type="AnalogueValue" />
      <DA bType="Quality" fc="MX" name="q" qchg="true" />
      <DA bType="Timestamp" fc="MX" name="t" />
      <DA bType="INT32U" dchg="true" fc="CF" name="db" />
      <DA bType="INT32U" dchg="true" fc="CF" name="zeroDb" />
      <DA bType="Struct" dchg="true" fc="CF" name="rangeC" type="RangeConfig" />
    </DOType>
    <DOType cdc="ENS" id="ENS_Health">
      <DA bType="Enum" dchg="true" fc="ST" name="stVal" type="HealthKind" />
      <DA bType="Quality" fc="ST" name="q" qchg="true" />
      <DA bType="Timestamp" fc="ST" name="t" />
    </DOType>
    <DOType cdc="LPL" id="LPL_NamPlt">
      <DA bType="VisString255" fc="DC" name="vendor" />
      <DA bType="VisString255" fc="DC" name="swRev" />
      <DA bType="VisString255" fc="DC" name="d" />
      <DA bType="VisString255" fc="DC" name="configRev" />
    </DOType>
    <DAType id="Originator">
      <BDA bType="Enum" name="orCat" type="orCat" />
      <BDA bType="Octet64" name="orIdent" />
    </DAType>
    <DAType id="ENCOperate">
      <BDA bType="Enum" name="ctlVal" type="tempEnum" />
      <BDA bType="Timestamp" name="operTm" />
      <BDA bType="Struct" name="origin" type="Originator" />
      <BDA bType="INT8U" name="ctlNum" />
      <BDA bType="Timestamp" name="T" />
      <BDA bType="BOOLEAN" name="Test" />
      <BDA bType="Check" name="Check" />
    </DAType>
    <DAType id="ENCCancel">
      <BDA bType="Enum" name="ctlVal" type="tempEnum" />
      <BDA bType="Timestamp" name="operTm" />
      <BDA bType="Struct" name="origin" type="Originator" />
      <BDA bType="INT8U" name="ctlNum" />
      <BDA bType="Timestamp" name="T" />
      <BDA bType="BOOLEAN" name="Test" />
    </DAType>
    <DAType id="Unit">
      <BDA bType="Enum" name="SIUnit" type="SIUnit" />
      <BDA bType="Enum" name="multiplier" type="multiplier" />
    </DAType>
    <DAType id="Vector">
      <BDA name="mag" bType="Struct" type="AnalogueValue" />
      <BDA name="ang" bType="Struct" type="AnalogueValue" />
    </DAType>
    <DAType id="AnalogueValue">
      <BDA bType="FLOAT32" name="f" />
    </DAType>
    <DAType id="ScaledValueConfig">
      <BDA bType="FLOAT32" name="scaleFactor" />
      <BDA bType="FLOAT32" name="offset" />
    </DAType>
    <DAType id="RangeConfig">
      <BDA bType="Struct" name="min" type="AnalogueValue" />
      <BDA bType="Struct" name="max" type="AnalogueValue" />
    </DAType>
    <DAType id="PulseConfig">
      <BDA bType="Enum" name="cmdQual" type="cmdQual" />
      <BDA bType="INT32U" name="onDur" />
      <BDA bType="INT32U" name="offDur" />
      <BDA bType="INT32U" name="numPls" />
    </DAType>
    <EnumType id="tempEnum">
      <EnumVal ord="0">e1</EnumVal>
      <EnumVal ord="1">e2</EnumVal>
      <EnumVal ord="2">e3</EnumVal>
      <EnumVal ord="3">e4</EnumVal>
      <EnumVal ord="4">e5</EnumVal>
    </EnumType>
    <EnumType id="TmSynEnum">
      <EnumVal ord="0">ExternalAreaClock</EnumVal>
      <EnumVal ord="1">LocalAreaClock</EnumVal>
      <EnumVal ord="2">GlobalAreaClock</EnumVal>
    </EnumType>
    <EnumType id="orCat">
      <EnumVal ord="0">not-supported</EnumVal>
      <EnumVal ord="1">bay-control</EnumVal>
      <EnumVal ord="2">station-control</EnumVal>
      <EnumVal ord="3">remote-control</EnumVal>
      <EnumVal ord="4">automatic-bay</EnumVal>
      <EnumVal ord="5">automatic-station</EnumVal>
      <EnumVal ord="6">automatic-remote</EnumVal>
      <EnumVal ord="7">maintenance</EnumVal>
      <EnumVal ord="8">process</EnumVal>
    </EnumType>
    <EnumType id="ctlModel">
      <EnumVal ord="0">status-only</EnumVal>
      <EnumVal ord="1">direct-with-normal-security</EnumVal>
      <EnumVal ord="2">sbo-with-normal-security</EnumVal>
      <EnumVal ord="3">direct-with-enhanced-security</EnumVal>
      <EnumVal ord="4">sbo-with-enhanced-security</EnumVal>
    </EnumType>
    <EnumType id="sboClass">
      <EnumVal ord="0">operate-once</EnumVal>
      <EnumVal ord="1">operate-many</EnumVal>
    </EnumType>
    <EnumType id="SIUnit">
      <EnumVal ord="1">none</EnumVal>
      <EnumVal ord="2">m</EnumVal>
      <EnumVal ord="3">kg</EnumVal>
      <EnumVal ord="4">s</EnumVal>
      <EnumVal ord="5">A</EnumVal>
      <EnumVal ord="6">K</EnumVal>
      <EnumVal ord="7">mol</EnumVal>
      <EnumVal ord="8">cd</EnumVal>
      <EnumVal ord="9">deg</EnumVal>
      <EnumVal ord="10">rad</EnumVal>
      <EnumVal ord="11">sr</EnumVal>
      <EnumVal ord="21">Gy</EnumVal>
      <EnumVal ord="22">q</EnumVal>
      <EnumVal ord="23">°C</EnumVal>
      <EnumVal ord="24">Sv</EnumVal>
      <EnumVal ord="25">F</EnumVal>
      <EnumVal ord="26">C</EnumVal>
      <EnumVal ord="27">S</EnumVal>
      <EnumVal ord="28">H</EnumVal>
      <EnumVal ord="29">V</EnumVal>
      <EnumVal ord="30">ohm</EnumVal>
      <EnumVal ord="31">J</EnumVal>
      <EnumVal ord="32">N</EnumVal>
      <EnumVal ord="33">Hz</EnumVal>
      <EnumVal ord="34">lx</EnumVal>
      <EnumVal ord="35">Lm</EnumVal>
      <EnumVal ord="36">Wb</EnumVal>
      <EnumVal ord="37">T</EnumVal>
      <EnumVal ord="38">W</EnumVal>
      <EnumVal ord="39">Pa</EnumVal>
      <EnumVal ord="41">m²</EnumVal>
      <EnumVal ord="42">m³</EnumVal>
      <EnumVal ord="43">m/s</EnumVal>
      <EnumVal ord="44">m/s²</EnumVal>
      <EnumVal ord="45">m³/s</EnumVal>
      <EnumVal ord="46">m/m³</EnumVal>
      <EnumVal ord="47">M</EnumVal>
      <EnumVal ord="48">kg/m³</EnumVal>
      <EnumVal ord="49">m²/s</EnumVal>
      <EnumVal ord="50">W/m K</EnumVal>
      <EnumVal ord="51">J/K</EnumVal>
      <EnumVal ord="52">ppm</EnumVal>
      <EnumVal ord="53">1/s</EnumVal>
      <EnumVal ord="54">rad/s</EnumVal>
      <EnumVal ord="61">VA</EnumVal>
      <EnumVal ord="62">Watts</EnumVal>
      <EnumVal ord="63">VAr</EnumVal>
      <EnumVal ord="64">theta</EnumVal>
      <EnumVal ord="65">cos(theta)</EnumVal>
      <EnumVal ord="66">Vs</EnumVal>
      <EnumVal ord="67">V²</EnumVal>
      <EnumVal ord="68">As</EnumVal>
      <EnumVal ord="69">A²</EnumVal>
      <EnumVal ord="70">A²t</EnumVal>
      <EnumVal ord="71">VAh</EnumVal>
      <EnumVal ord="72">Wh</EnumVal>
      <EnumVal ord="73">VArh</EnumVal>
      <EnumVal ord="74">V/Hz</EnumVal>
    </EnumType>
    <EnumType id="multiplier">
      <EnumVal ord="-24">Yocto</EnumVal>
      <EnumVal ord="-21">Zepto</EnumVal>
      <EnumVal ord="-18">Atto</EnumVal>
      <EnumVal ord="-15">Femto</EnumVal>
      <EnumVal ord="-12">Pico</EnumVal>
      <EnumVal ord="-9">Nano</EnumVal>
      <EnumVal ord="-6">Micro</EnumVal>
      <EnumVal ord="-3">Milli</EnumVal>
      <EnumVal ord="-2">Centi</EnumVal>
      <EnumVal ord="-1">Deci</EnumVal>
      <EnumVal ord="0">zeroNoValue</EnumVal>
      <EnumVal ord="1">Deca</EnumVal>
      <EnumVal ord="2">Hecto</EnumVal>
      <EnumVal ord="3">Kilo</EnumVal>
      <EnumVal ord="6">Mega</EnumVal>
      <EnumVal ord="9">Giga</EnumVal>
      <EnumVal ord="12">Tera</EnumVal>
      <EnumVal ord="15">Petra</EnumVal>
      <EnumVal ord="18">Exa</EnumVal>
      <EnumVal ord="21">Zetta</EnumVal>
      <EnumVal ord="24">Yotta</EnumVal>
    </EnumType>
    <EnumType id="range">
      <EnumVal ord="0">normal</EnumVal>
      <EnumVal ord="1">high</EnumVal>
      <EnumVal ord="2">low</EnumVal>
      <EnumVal ord="3">high-high</EnumVal>
      <EnumVal ord="4">low-low</EnumVal>
    </EnumType>
    <EnumType id="cmdQual">
      <EnumVal ord="0">pulse</EnumVal>
      <EnumVal ord="1">persistent</EnumVal>
    </EnumType>
    <EnumType id="HealthKind">
      <EnumVal ord="1">Ok</EnumVal>
      <EnumVal ord="2">Warning</EnumVal>
      <EnumVal ord="3">Alarm</EnumVal>
    </EnumType>
    <EnumType id="BehKind">
      <EnumVal ord="1">on</EnumVal>
      <EnumVal ord="2">blocked</EnumVal>
      <EnumVal ord="3">test</EnumVal>
      <EnumVal ord="4">test/blocked</EnumVal>
      <EnumVal ord="5">off</EnumVal>
    </EnumType>
    <EnumType id="ModKind">
      <EnumVal ord="1">on</EnumVal>
      <EnumVal ord="2">blocked</EnumVal>
      <EnumVal ord="3">test</EnumVal>
      <EnumVal ord="4">test/blocked</EnumVal>
      <EnumVal ord="5">off</EnumVal>
    </EnumType>
  </DataTypeTemplates>
</SCL>